{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["BoM","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BoM","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[[1,1,1,11]]}
[]
[null,"Project components for 1 prototype"]
[]
[]
[]
[]
[null,null,"Prototype quantity :",10]
[null,"Item","Schematics Ref","Qty","Price/chip","Total price","Stock","Description","Manufacturer P/N","Manufacturer","Packaging","Internet link"]
[null,1,"U2",1,4.53,{"$f":"D9*E9","v":4.53},208,"IC HOT-SWAP CTRLR N-CH 10-UMAX","MAX5925DEUB+","Maxim Integrated","10-uMAX","http://www.digikey.com/product-detail/en/MAX5925DEUB%2B/MAX5925DEUB%2B-ND/1937487"]
[null,2,"U6",1,9.8800000000000008,{"$f":"D10*E10","v":9.8800000000000008},1727,"IC REG BUCK SYNC 3.3V/ADJ 16QSOP","MAX1685EEE+","Maxim Integrated","16-QSOP","http://www.digikey.com/product-detail/en/MAX1685EEE%2B/MAX1685EEE%2B-ND/947774"]
[null,3,"U7",1,8.44,8.44,1372,"IC MCU 32BIT 256KB FLASH 100LQFP","ATSAM3U4CA-AU","Atmel","100-LQFP","http://www.digikey.com/product-detail/en/ATSAM3U4CA-AU/ATSAM3U4CA-AU-ND/2177035"]
[null,4,"a b",2,0.39900000000000002,0.79800000000000004,16120,"RES 100 OHM 1W 1% 2512 SMD","CRCW2512100RFKEG","Vishay Dale","2512 (6332 Metric)","http://www.digikey.com/product-detail/en/CRCW2512100RFKEG/541-100AFCT-ND/1178705"]
[null,5,"c d e",3,0.28899999999999998,0.86699999999999999,12252,"RES 49.9 OHM 1/2W 1% 1210 SMD","CRCW121049R9FKEA","Vishay Dale","1210 (3225 Metric)","http://www.digikey.com/product-detail/en/CRCW121049R9FKEA/541-49.9AACT-ND/1182399"]
[null,6,null,0,2.67,0,6848,"IC OPAMP RRIO ZERO DRIFT SC70-5","ADA4051-1AKSZ-R7","Analog Devices Inc","SC-70-5","http://www.digikey.com/product-detail/en/ADA4051-1AKSZ-R7/ADA4051-1AKSZ-R7CT-ND/2264661"]
[null,7,null,0,7.38,0,814,"IC DAC 10BIT OCTAL R-R 16-TSSOP","DAC108S085CIMT/NOPB","National Semiconductor","16-TSSOP","http://www.digikey.com/product-detail/en/DAC108S085CIMT%2FNOPB/DAC108S085CIMT-ND/1658142"]
[null,8,null,0,4.3600000000000003,0,10220,"RES NET 25K OHM 2 RES TO-236-3","MPMT5002AT1","Vishay Thin Film","TO-236","http://www.digikey.com/product-detail/en/MPMT5002AT1/MPMT-25K%2F25KCT-ND/1771077"]
[null,9,null,0,2.21,0,7140,"IC REG LDO 10V 1A SOT223-4","LM2940IMP-10/NOPB","National Semiconductor","SOT-223-3","http://www.digikey.com/product-detail/en/LM2940IMP-10%2FNOPB/LM2940IMP-10CT-ND/363885"]
[null,10,null,0,2.15,0,21889,"IC VREF SERIES PREC 2.5V SOT23-3","AD1582BRTZ-REEL7","Analog Devices Inc","SOT-23-3","http://www.digikey.com/product-detail/en/AD1582BRTZ-REEL7/AD1582BRTZREEL7CT-ND/751229"]
[null,11,null,0,9.8800000000000008,0,1727,"IC REG BUCK SYNC 3.3V/ADJ 16QSOP","MAX1685EEE+","Maxim Integrated","16-QSOP","http://www.digikey.com/product-detail/en/MAX1685EEE%2B/MAX1685EEE%2B-ND/947774"]
[null,null,"Total:",{"$f":"SUM(D9:D19)","v":8},null,{"$f":"SUM(F9:F19)","v":24.515000000000004}]
[null,null,"Total for 100 prototypes :",null,null,12.179449999999999]
[null,null,"Total for 1000 prototypes :",null,null,11.185060000000002]
[null,null,"Total for 5000 prototypes :",null,null,11.185060000000002]
[null," ","Total for 10k \"prototypes\" :",null,null,11.185060000000002]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}