{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["BoM","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BoM","index":0,"n_rows":27,"n_cols":12,"rows_kept":27,"cut":false,"hidden":false,"merged":[[1,1,1,11]]}
[]
[null,"Project components for 1 prototype"]
[]
[]
[]
[]
[null,null,"Prototype quantity :",5]
[null,"Item","Schematics Ref","Qty","Price/chip","Total price","Stock","Description","Manufacturer P/N","Manufacturer","Packaging","Internet link"]
[null,1,"U1",1,2.73,{"$f":"D9*E9","v":2.73},12858,"IC OPAMP GP R-R 50MHZ DUAL 8SOIC","OPA2365AIDR","Texas Instruments","8-SOIC","http://www.digikey.com/product-detail/en/OPA2365AIDR/296-31704-1-ND/3505181"]
[null,2,"U2",1,0.94,{"$f":"D10*E10","v":0.94},3452,"IC COMPARATOR VOLT SGL SOT23-5","MAX9031AUK+T","Maxim Integrated","SOT-23-5","http://www.digikey.com/product-detail/en/MAX9031AUK%2BT/MAX9031AUK%2BTCT-ND/774161"]
[null,3,"D1",1,0.46,{"$f":"D11*E11","v":0.46},12215,"DIODE SCHOTTKY 30V 1A SMA","STPS1L30A","STMicroelectronics","SMA","http://www.digikey.com/product-detail/en/STPS1L30A/497-6577-1-ND/1865323"]
[null,4,"P1 P2 P3 P4",4,0.20499999999999999,{"$f":"D12*E12","v":0.82},27567,"CONN HEADER 2POS .100 VERT TIN",22032021,"Molex Inc",null,"http://www.digikey.com/product-detail/en/0022032021/WM4000-ND/26623"]
[null,5,"C1 C10",2,4.5999999999999999E-2,{"$f":"D13*E13","v":9.1999999999999998E-2},2197931,"CAP CER 0.1UF 50V 10% X7R 0805","GRM21BR71H104KA01L","Murata Electronics North America","0805 (2012 Metric)","http://www.digikey.com/product-detail/en/GRM21BR71H104KA01L/490-1666-1-ND/587431"]
[null,6,"C6 C7",2,4.1000000000000002E-2,{"$f":"D14*E14","v":8.2000000000000003E-2},34304,"CAP CER 2200PF 50V 10% X7R 0805","C0805C222K5RACTU","Kemet","0805 (2012 Metric)","http://www.digikey.com/product-detail/en/C0805C222K5RACTU/399-1151-1-ND/411426"]
[null,7,"C4 C5 C8",3,0.22500000000000001,{"$f":"D15*E15","v":0.67500000000000004},383223,"CAP CER 4.7UF 25V 10% X5R 0805","GRM21BR61E475KA12L","Murata Electronics North America","0805 (2012 Metric)","http://www.digikey.com/product-detail/en/GRM21BR61E475KA12L/490-3335-1-ND/702876"]
[null,8,"C11 C2 C3 C9",4,0.14399999999999999,{"$f":"D16*E16","v":0.57599999999999996},112273,"CAP CER 10UF 10V 10% X5R 0805","GRM21BR61A106KE19L","Murata Electronics North America","0805 (2012 Metric)","http://www.digikey.com/product-detail/en/GRM21BR61A106KE19L/490-1709-1-ND/587432"]
[null,9,"R8 R11",2,0.1,{"$f":"D17*E17","v":0.2},52297,"RES 8.2K OHM 1/8W 1% 0805 SMD","ERJ-6ENF8201V","Panasonic Electronic Components",805,"http://www.digikey.com/product-detail/en/ERJ-6ENF8201V/P8.20KCCT-ND/1746897"]
[null,10,"R1 R2 R5 R9 R10",5,0.1,{"$f":"D18*E18","v":0.5},7719145,"RES 10K OHM 1/8W 1% 0805 SMD","ERJ-6ENF1002V","Panasonic Electronic Components",805,"http://www.digikey.com/product-detail/en/ERJ-6ENF1002V/P10.0KCCT-ND/119248"]
[null,11,"R3",1,0.1,{"$f":"D19*E19","v":0.1},62736,"RES 12K OHM 1/8W 1% 0805 SMD","ERJ-6ENF1202V","Panasonic Electronic Components",805,"http://www.digikey.com/product-detail/en/ERJ-6ENF1202V/P12.0KCCT-ND/1746818"]
[null,12,"R4",1,0.1,{"$f":"D20*E20","v":0.1},83033,"RES 330K OHM 1/8W 1% 0805 SMD","RC0805FR-07330KL","Yageo",805,"http://www.digikey.com/product-detail/en/RC0805FR-07330KL/311-330KCRCT-ND/730814"]
[null,13,"R6 R7",2,0.1,{"$f":"D21*E21","v":0.2},217660,"RES 1M OHM 1/8W 1% 0805 SMD","ERJ-6ENF1004V","Panasonic Electronic Components",805,"http://www.digikey.com/product-detail/en/ERJ-6ENF1004V/P1.00MCCT-ND/119836"]
[null,14,"FB1",1,0.1,{"$f":"D22*E22","v":0.1},300534,"FERRITE CHIP SIGNAL 1000 OHM SMD","HZ0805D102R-10","Laird-Signal Integrity Products","0805 (2012 Metric)","http://www.digikey.com/product-detail/en/HZ0805D102R-10/240-2397-1-ND/806757"]
[null,null,"Total:",{"$f":"SUM(D9:D22)","v":30},null,{"$f":"SUM(F9:F22)","v":7.5749999999999984}]
[null,null,"Total for 100 prototypes :",null,null,4.1819799999999994]
[null,null,"Total for 1000 prototypes :",null,null,2.8910900000000002]
[null,null,"Total for 5000 prototypes :",null,null,2.8763299999999994]
[null," ","Total for 10k \"prototypes\" :",null,null,2.8763299999999994]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}