{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["BoM","Feuil2","Feuil3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BoM","index":0,"n_rows":33,"n_cols":16,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,1,1,12]]}
[]
[null,"Project Bill Of Materials"]
[]
[]
[]
[]
[null,null,"Prototype quantity :",3]
[null,"Item","Schematics Ref","Qty","Price/chip","Total Price","Home Stock","Digikey Stock","Description","Manufacturer P/N","Manufacturer","Packaging","Internet link","Category","Family","(Value)"]
[null,1,"U1",1,null,null,null,null,"IC REG LDO 3.3V 1A SOT223","NCP1117LPST33T3G","ON Semi","SOT-223","http://www.digikey.com/product-detail/en/NCP1117LPST33T3G/NCP1117LPST33T3GOSCT-ND/3462387"]
[null,2,"U3",1,null,null,null,null,"IC USB SERIAL BASIC UART 16SSOP","FT230XS-R","FTDI","SSOP16","http://www.digikey.com/product-detail/en/FT230XS-R/768-1135-1-ND/3029155"]
[null,{"$f":"B10+1","v":3},"CON1",1,null,null,null,null,"CONN USB MICRO B RECPT SMT R/A","10118194-0001LF","FCI",null,"http://www.digikey.com/product-detail/en/10118194-0001LF/609-4618-1-ND/2785382"]
[null,{"$f":"B11+1","v":4},"Q2",1,null,null,null,null,"MOSFET N (VGSth < 2V!) SOT23"]
[null,5,"Q1",1,null,null,null,null,"MOSFET P (VGSth < 2V!) SOT23"]
[null,6,"P1",1,null,null,null,null,"CONN FEMALE 12POS .1\" SMD TIN","NPTC121KFXC-RC","Sulins Connector Solutions",null,"http://www.digikey.com/product-detail/en/NPTC121KFXC-RC/S5604-ND/776062"]
[null,7,"SW1",1,null,null,null,null,"SWITCH TACTILE SPST-NO 0.05A 12V","PTS645SM43SMTR92 LFS","C&K",null,"http://www.digikey.com/product-detail/en/PTS645SM43SMTR92%20LFS/CKN9112CT-ND/1146934"]
[null,8,"C5 C6",2,null,null,null,null,"CAP 47pF 0603 >=6.3V"]
[null,9,"C4 C7 C8",3,null,null,null,null,"CAP 100nF 0603 >=6.3V"]
[null,10,"C1 C2 C3 C9 C10",5,null,null,null,null,"CAP 4,7uF 0603 >= 6,3V"]
[null,11,"D1 D2 D3",3,null,null,null,null,"LED 0603 GREEN"]
[null,12,"FB1",1,null,null,null,null,"FERRITE 0603"]
[null,13,"R3",1,null,null,null,null,"RES 0Ohms 0603"]
[null,14,"R6 R7",2,null,null,null,null,"RES 27Ohms 0603"]
[null,15,"R1 R2 R4 R9 R10 R11",6,null,null,null,null,"RES 1k 0603"]
[null,16,"R5",1,null,null,null,null,"RES ARRAY 1K OHM 8 RES 2506","742C163102JP",null,null,"http://www.digikey.com/product-detail/en/742C163102JP/742C163102JPCT-ND/1124513"]
[null,17,"R8",1,null,null,null,null,"NOT POPULATED"]
[null,18,"U4",1,null,null,null,null,"BREADBOARD SOLDERLESS (TAPED ON BOARD)",null,null,null,"http://www.digikey.com/product-detail/en/700-00012/700-00012-ND/1774444"]
[null,19,"U2",1,null,null,null,null,"ESP8266 module - ESP-03",null,null,null,"http://www.ebay.com/itm/ESP8266-Serial-Wireless-WIFI-Transceiver-Module-Send-Receive-LWIP-AP-STA-A-/201206173209"]
[null,null,"Total:",{"$f":"SUM(D9:D27)","v":34},null,{"$f":"SUM(F9:F27)","v":0}]
[null,null,"Total for 10 prototypes :",null,null,0]
[null,null,"Total for 100 prototypes :",null,null,0,null,"Missing in Kicad: "]
[null,null,"Total for 1000 prototypes :",null,null,0,null,"Missing in BoM:"]
[null,null,"Total for 5000 prototypes :",null,null,0]
[null," ","Total for 10k \"prototypes\" :",null,null,0]

{"sheet":"Feuil2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Feuil3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}